**Standard delivery:**

* Compact and versatile cookware, dishware and glassware washing machine - Automatic hood lift operated by the hands-free foot mechanism or by push on the operating panel - Safety crush protection and detection of obstacles - Manual override for the hood by the stainless-steel ergonomic handle if electrical breakdown.
* Can be installed along a wall or at a corner - Operating panel positioned at eye level and installable on site on right or left side.
* Stainless steel construction - Rear cover plate - Hood double skinned - Noise & heat insulated hood.
* Liquid detergent and rinse aid dosing dispenser with peristaltic pump - Suction hoses - Prepared to detergent dosing sensor installation.
* Drain and discharge pump with water drain lifting height of 800 mm.
* Basket loading size: 500 x 500 mm - Removable rack holder - Clear passing height: 430 mm - Working height: 860 - 910 mm.
* QR code with immediate online access to operator training videos - servicing history - troubleshooting guides.
* Wifi connectivity preparation: HACCP Data collection and history - Control of washing parameters - Tele service with detection of defective component - Apps to load on Google Play or Apps Store.
* Starter kit: 1 Stainless steel cookware wash basket - 1 Polypropylene dishware wash basket - 1 Polypropylene glassware wash basket.
* Installation kit: Supply hose 3/4" female - Drain hose Ø 28 mm - 2 m. electrical cable.

**Efficient washing and rinsing technology:**

* Automatic activation of wash mode by wash basket detection sensor.
* Cookware washing technology: 2 Stainless steel oscillating arms driven by motor and removable without tool and positioned below the wash basket - Stainless steel nozzles - 1 High pressure wash pump 1,5 kW.
* Dishware and Glassware washing technology: 2 Stainless steel rotating arms driven by water pressure and removable without tool - 1 over the wash basket, 1 below - Printed nozzles - 1 Low pressure wash pump 1,1 kW.
* Rinsing technology: 2 Stainless steel arms removable without tool and with optimized pressure system - 1 over the washing basket, 1 below - Stainless steel nozzles - 1 rinse pump 0,18 kW.
* Stamped wash tank without any welding: 30 L - 2 stage filter system - Heating element 8 kW.
* Rinse tank: 12 L - Heating element 8 kW.

**User benefits:**

* Easy to use operating panel with washing program icons, count down, wash and rinse tank temperature.
* Intuitive operating panel with waterproof colored TFT screen display within easy reach.
* Total starting time (Fill and heat water): 9 min. with 55°C water inlet.
* Water change time (Drain, fill and heat): 5 min. with 55°C water inlet.
* Cookware wash mode - 2 programs: 3 min.(cookware) - 6 min. (carbonized cookware) .
* Dishware and Glassware wash mode - 2 programs: 2 min. (plates, cutlery, utensils) - 1 min. (glasses).
* Self-cleaning program.
* Auto start wash cycle.
* Wash temperature: Factory setting 60°C - Adjustable from 35°C up to 65°C for each wash program independently.
* Rinse temperature: Factory setting 85°C - Adjustable from 65°C up to 85°C for each wash program independently.
* Programmable shutdown timer.

**Capacity per wash cycle:**

* Cookware wash mode: Pot up to Ø 450 H 380 mm or sub sized - 1 GN 1/1 Depth 200 mm or sub-sized - 2 GN 1/1 Depth 65 mm.
* Dishware and Glassware wash mode: 18 Dinner plates or 12 Soup plates Ø 240 mm - 25 Glasses/mugs ∅ 90 mm.

**Consumptions per wash cycle:**

* Water: 2.6 L – Energy 0.176 kWh.
* Water and energy consumption management - Energy saving mode if not used for 20 min.

**Dimensions - Connections - Standards and certification compliance:**

* Dimension: H 1950 mm x W (655+100 handle) x D (785+95 handle) - Side operating panel L 430 mm.
* Weight: Net 150 Kg, Gross 190 Kg.
* Water inlet: 55°C/60°C - 2-5 bar - < 4 °Dh (7 °f) - 70 PPM - 3/4" female. - Water outlet: Ø 28 mm - 65°C - ⩾ 50 L/min.
* Connected load: 16 A - 10 kW - 3N AC 380-400-415 V - 50 Hz.
* < 64 dB(A) - IPX5 - CE - DIN 10534 - EN 1717 - RoHS - WEEE.

**Factory fitted options:**

* **Other voltage and frequency:** 27 A - 10 kW - 3N AC 230 V - 50 Hz.
* **Inbuilt exhaust heat recovery with steam condensing unit** - Self-cleaning function - 10°C/25°C water supply - Wash cycle extended of 30 sec. - Dimension of the machine equipped of the option: H 2125 mm x W (655+100 handle) x D (785+95 handle).

**Water treatment option:**

* **Non-electric external water softener**: 2°C /65°C Water supply - 8 kg Salt capacity - Regeneration cycle at 2 bar: water 34 L, time 11 min Dimension: H 500 x L 200 mm x D 450 mm - Weight: Net 21 Kg, Gross 39 Kg - Water connection: Inlet 3/4" male, Outlet 3/4" male, Drain 1/2".

**High productivity options:**

* **Pots and pans scrubber with ergonomic handle** - Thermal resistant to 100°C - Dimension: L 101 x D 152 x H 76 mm - Packing 12 units.
* **Stainless steel cookware wash basket** - L 500 x D 500 x H 85 mm - Capacity: Pot up to Ø 450 H 380 mm or sub sized - 1 GN 1/1 Depth 200 mm or sub-sized - 2 GN 1/1 Depth 65 mm.
* **Polypropylene dishware wash basket** - L 500 x D 500 x H 110 mm - Capacity: 18 Dinner plates or 12 Soup plates Ø 240 mm.
* **Polypropylene glassware wash basket** - L 500 x D 500 x H 118 mm - Capacity: 25 Glasses or mugs ∅ 90 mm.
* **Polypropylene cutlery wash holder** - L 105 x D 105 x H 140 mm - Fits with polypropylene dishware wash basket.